{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-A9"]
[]
[]
[]
[]
["","","","","","3MXM40A2V1B9","3MXM52A2V1B9","3MXM68A2V1B9"]
["Димензии","Единица","","Висина","mm","734","734","734"]
["","","","Ширина","mm","974","974","974"]
["","","","Длабочина","mm","408","408","408"]
["Тежина","Единица","","","kg","57","57","62"]
["Компресор","Тип","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","-10","-10"]
["","","","Max.","°CDB","46","46","46"]
["Sound pressure level","Cooling","","Nom.","dBA","46","46","48"]
["","Heating","","Nom.","dBA","47","47","48"]
["Разладно средство","Тип","","","","R-32","R-32","R-32"]
["","Полнење","","","kg","1.8","1.8","2"]
["Refrigerant","Charge","","","tCO2Eq","1.22","1.22","1.35"]
["Разладно средство","GWP","","","","675","675","675"]
["Piping connections","Piping length","OU - IU","Max.","m","25 (1)","25 (1)","25 (1)"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)","0.02 (for piping length exceeding 30m)","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","m","15","15","15"]
["","","IU - IU","Max.","m","7.5","7.5","7.5"]
["","Total piping length","System","Actual","m","50 (2)","50 (2)","50"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["","Reducer assembly","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Напојување со струја","Фаза","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - For one room","(1) - For one room"]
["","","","","","(2) - За комбинација со CVXM-A, FVXM-A - максималната должина на цевки е 30 m.","(2) - За комбинација со CVXM-A, FVXM-A - максималната должина на цевки е 30 m."]
["","","","","","","","(1) - For one room"]