{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-A"]
[]
[]
[]
[]
["","","","","","4MXM68A2V1B","4MXM80A2V1B"]
["Димензии","Единица","","Висина","mm","734","734"]
["","","","Ширина","mm","974","974"]
["","","","Длабочина","mm","408","408"]
["Тежина","Единица","","","kg","63","67"]
["Компресор","Тип","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["Sound pressure level","Cooling","","Nom.","dBA","48","48"]
["","Heating","","Nom.","dBA","49","49"]
["Разладно средство","Тип","","","","R-32","R-32"]
["","Полнење","","","kg","2","2.4"]
["Refrigerant","Charge","","","tCO2Eq","1.35","1.62"]
["Разладно средство","GWP","","","","675","675"]
["Piping connections","Piping length","OU - IU","Max.","m","25 (1)","25 (1)"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","m","15","15"]
["","","IU - IU","Max.","m","7.5","7.5"]
["","Total piping length","System","Actual","m","60","70"]
["Standard Accessories","Прирачник за инсталирање","","","","1","1"]
["","Капаче за одвод","","","","3","3"]
["","Приклучок за одвод","","","","1","1"]
["","Склоп за редуцир","","","","1","1"]
["","Кесичка со завртки","","","","1","1"]
["Опсег на енергетска ефикасност","","","","","A+++ ~ D","A+++ ~ D"]
["Напојување со струја","Фаза","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - For one room","(1) - For one room"]
["","","","","","(2) - See separate drawing for operation range","(2) - See separate drawing for operation range"]
["","","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]
["","","","","","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases"]