{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELBH-E6V"]
[]
[]
[]
[]
["","","","","","ELBH12EF6V"]
["Куќиште","Боја","","","","White + Black"]
["","Материјал","","","","Resin, sheet metal"]
["Димензии","Единица","","Висина","mm","840"]
["","","","Ширина","mm","440"]
["","","","Длабочина","mm","390"]
["Тежина","Единица","","","kg","48.5"]
["PED","Категорија","","","","Category II"]
["Sound power level","Nom.","","","dBA","44.0"]
["Sound pressure level","Nom.","","","dBA","30.0"]
["Operation range","Heating","Water side","Min.","°C","15"]
["","","","Max.","°C","65"]
["","Cooling","Ambient","Min.","°CDB","10"]
["","","Water side","Min.","°C","5"]
["","","","Max.","°C","22"]
["Напојување со струја","Име","","","","See note 6"]
["Electric heater","Power supply","","Name","","6V3"]
["","","","Phase","","1~ / 3~"]
["","","","Frequency","Hz","50"]
["","","","Voltage","V","230"]
["","Recommended fuses","","","A","20.000"]
["Notes","","","","","(1) - Работниот простор е проширен за да се намали брзината на протокот, во зависност од режимот на работа - погледнете ја кривата ESP."]
["","","","","","(2) - Excluding the water volume in the unit. This volume will guarantee suficient defrost energy for all applications, however, this volume can be multiplied by 0,66 if the heating sepoint is ≥ 45° C (eg. Fan coils)"]
["","","","","","(3) - Measured with a pressure drop of 10 kPa in the heating system at an operating condition of leaving water 47-55°C in a room with an ambient of 20°C. DB/WB 7°C/6°."]
["","","","","","(4) - Sound values are measured in a semi-anechoic room. Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings. Sound power level is an absolute value that a so"]
["","","","","","(5) - For more details, see operation range drawing"]
["","","","","","(6) - 4 pole 20 A curve 400V tripping class C (refer to wiring diagram)"]