{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":8,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERRA08-12EV3"]
[]
[]
[]
[]
["","","","","","ERRA08EAV3","ERRA10EAV3","ERRA12EAV3"]
["Димензии","Единица","","Висина","mm","1,003","1,003","1,003"]
["","","","Ширина","mm","1270","1270","1270"]
["","","","Длабочина","mm","533","533","533"]
["Тежина","Единица","","","kg","107","107","107"]
["Fan","Air flow rate","Heating","High","m³/min","89.9","89.9","89.9"]
["","","Cooling","High","m³/min","80.1","80.1","80.1"]
["Operation range","Cooling","","Min.","°CDB","10","10","10"]
["","","","Max.","°CDB","43","43","43"]
["","Domestic hot water","","Min.","°CDB","-25","-25","-25"]
["","","","Max.","°CDB","35","35","35"]
["Sound power level","Heating","","Nom.","dBA","56.0","56.0","56.0"]
["","Cooling","","Nom.","dBA","60.1","60.6","61.5"]
["Sound pressure level","Heating","","Nom.","dBA","40.6","40.6","40.6"]
["","Cooling","","Nom.","dBA","47","47.4","48.5"]
["Разладно средство","Тип","","","","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0"]
["Refrigerant","Charge","","","tCO2Eq","2.19","2.19","2.19"]
["Разладно средство","Полнење","","","kg","3.25","3.25","3.25"]
["Поврзувања на цевките","Течност","","OD","mm","6.35","6.35","6.35"]
["","Гас","","OD","mm","15.9","15.9","15.9"]
["Piping connections","Level difference","IU - OU","Max.","m","30.0","30.0","30.0"]
["Напојување со струја","Име","","","","V3","V3","V3"]
["","Фаза","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","230","230","230"]
["Current","Recommended fuses","","","A","32","32","32"]
["Notes","","","","","(1) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["","","","","","(3) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(3) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(3) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","","(4) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta 35°C - LWE 7°C ( DT =","(4) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta 35°C - LWE 7°C ( DT =","(4) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta 35°C - LWE 7°C ( DT ="]