{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":12,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / 2MXM-A9"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B9 / FDXM25F3V1B9 / 2MXM50A2V1B9","FDXM25F3V1B9 / FDXM25F3V1B9 / 2MXM40A2V1B9","FDXM25F3V1B9 / FDXM35F3V1B9 / 2MXM40A2V1B9","FDXM25F3V1B9 / FDXM35F3V1B9 / 2MXM50A2V1B9","FDXM25F3V1B9 / FDXM50F3V1B9 / 2MXM50A2V1B9","FDXM35F3V1B9 / FDXM35F3V1B9 / 2MXM50A2V1B9","FDXM35F3V1B9 / FDXM50F3V1B9 / 2MXM50A2V1B9","FDXM35F3V1B9 / FDXM35F3V1B9 / 2MXM68A2V1B9"]
["Cooling capacity","Nom.","","kW","5.00","","","","","","","6.8"]
["Heating capacity","Nom.","","kW","5.60","","","","","","","8.60"]
["Nominal efficiency","EER","","","3.21","","","","","","","2.73"]
["","COP","","","3.66","","","","","","","3.01"]
["","Annual energy consumption","","kWh","779","","","","","","","1245"]
["","Energy labeling Directive","Cooling","","A"]
["","","Heating","","A"]
["Space cooling","Energy efficiency class","","","A++","","","","","","","A"]
["","Capacity","Pdesign","kW","5.00","","","","","","","6.80"]
["","SEER","","","6.22","","","","","","","5.43"]
["","Annual energy consumption","","kWh/a","281","","","","","","","438"]
["Space heating (Average climate)","Energy efficiency class","","","A","","","","","","","A"]
["","Capacity","Pdesign","kW","4.20","","","","","","","3.60"]
["","SCOP/A","","","3.80","","","","","","","3.81"]
["","Pdh Heating capacity at -10°","","kW","2.92","","","","","","","3.10"]
["","Annual energy consumption","","kWh/a","1548","","","","","","","1323"]
["Опсег на енергетска ефикасност","","","","A+++ ~ D","","","","","","","A+++ ~ D"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Cooling capacity","Nom.","","kW","","4.00","4.00","5.00","5.00","5.00","5.00"]
["Heating capacity","Nom.","","kW","","4.20","4.20","5.60","5.60","5.60","5.60"]
["Nominal efficiency","Annual energy consumption","","kWh","","563","556","769","712","760","704"]
["","COP","","","","4.13","4.17","3.64","3.61","3.62","3.61"]
["","EER","","","","3.55","3.60","3.25","3.51","3.29","3.55"]
["","Energy labeling Directive","Cooling","","","A","A","A","A","A","A"]
["","","Heating","","","A","A","A","A","A","A"]
["Space cooling","Annual energy consumption","","kWh/a","","223","228","280","269","273","273"]
["","Energy efficiency class","","","","A++","A++","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","","4.00","4.00","5.00","5.00","5.00","5.00"]
["","SEER","","","","6.28","6.16","6.25","6.52","6.42","6.40"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","","1,117","1,106","1,548","1,529","1,544","1,514"]
["","Capacity","Pdesign","kW","","3.20","3.20","4.20","4.20","4.20","4.20"]
["","Energy efficiency class","","","","A+","A+","A","A","A","A"]
["","Pdh Heating capacity at -10°","","kW","","2.61","2.62","2.94","3.27","2.98","3.31"]
["","SCOP/A","","","","4.01","4.05","3.80","3.85","3.81","3.88"]