{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":10,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CS"]
[]
[]
[]
[]
["","","","","","FTXA20C2V1BS","FTXA25C2V1BS","FTXA35C2V1BS","FTXA42C2V1BS","FTXA50C2V1BS"]
["Power input","Cooling","","Nom.","kW","0.02","0.022","0.023","0.028","0.030"]
["","Heating","","Nom.","kW","0.02","0.02","0.22","0.036","0.039"]
["Куќиште","Боја","","","","Silver","Silver","Silver","Silver","Silver"]
["Димензии","Единица","","Висина","mm","295","295","295","295","295"]
["","","","Ширина","mm","798","798","798","798","798"]
["","","","Длабочина","mm","189","189","189","189","189"]
["Тежина","Единица","","","kg","11.5","11.5","11.5","11.5","11.5"]
["Fan","Air flow rate","Cooling","High","m³/min","11","11.5","11.9","13.1","13.5"]
["","","","Medium","m³/min","8.2","8.6","8.6","9.8","10.4"]
["","","","Low","m³/min","6.1","6.1","6.1","7.2","7.6"]
["","","","Silent operation","m³/min","4.6","4.6","4.6","4.6","5.2"]
["","","Heating","High","m³/min","10.9","11.1","11.5","14.6","15.1"]
["","","","Medium","m³/min","8.7","9","9","10.5","11.1"]
["","","","Low","m³/min","6.4","6.4","6.4","7.7","8.2"]
["","","","Silent operation","m³/min","4.5","4.5","4.5","5.2","5.7"]
["Sound power level","Cooling","","","dBA","57","57","60","60","60"]
["Sound pressure level","Cooling","","High","dBA","39","40","41","45","46"]
["","","","Medium","dBA","32","33","33","37","39"]
["","","","Low","dBA","25","25","25","29","31"]
["","","","Silent operation","dBA","19","19","19","21","24"]
["","Heating","","High","dBA","39","40","41","45","46"]
["","","","Medium","dBA","32","33","33","37","42"]
["","","","Low","dBA","25","25","25","29","33"]
["","","","Silent operation","dBA","19","19","19","21","24"]
["Разладно средство","GWP","","","","675","675","675","675","675.0"]
["Поврзувања на цевките","Течност","","OD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Гас","","OD","mm","9.5","9.5","9.5","9.5","12.70"]
["","Одвод","","","","18","18","18","18","18"]
["Контролни системи","Инфрацрвен далечински управувач","","","","ARC466A85","ARC466A85","ARC466A85","ARC466A85","ARC466A85"]
["","Жичен далечински управувач","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1"]
["","Screw cover","","","","2","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","Air filter","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Remote controller mounting plate","","","","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1"]
["Напојување со струја","Име","","","","V1","V1","V1","V1","V1"]
["","Фаза","","","","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240"]