{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-A / RZAG-A"]
[]
[]
[]
[]
["","","","","FTXM35A5V1B / RZAG35A2V1B","FTXM35A2V1B / RZAG35A2V1B","FTXM50A5V1B / RZAG35A2V1B","FTXM50A2V1B / RZAG35A2V1B","FTXM50A5V1B / RZAG50A2V1B","FTXM50A2V1B / RZAG50A2V1B"]
["Cooling capacity","Min.","","kW","1.60","1.60","1.60","1.60","1.70","1.70"]
["","Nom.","","kW","3.50","3.50","3.50","3.50","5.00","5.00"]
["","Max.","","kW","5.00","5.00","5.00","5.00","6.00","6.00"]
["Heating capacity","Min.","","kW","1.40","1.40","1.40","1.40","1.50","1.50"]
["","Nom.","","kW","4.00","4.00","4.00","4.00","6.00","6.00"]
["","Max.","","kW","5.30","5.30","5.30","5.30","6.50","6.50"]
["Nominal efficiency","EER","","","4.30","4.30","4.32","4.32","4.00","4.00"]
["","COP","","","3.85","3.85","3.93","3.93","4.00","4.00"]
["","Annual energy consumption","","kWh","407","407","405","405","625","625"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A"]
["Space cooling","Energy efficiency class","","","A++","A++","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","3.50","3.50","3.50","3.50","5.00","5.00"]
["","SEER","","","7.70","7.70","7.76","7.76","7.41","7.41"]
["","Annual energy consumption","","kWh/a","159","159","158","158","236","236"]
["Space heating (Average climate)","Energy efficiency class","","","A++","A++","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","2.60","2.60","2.60","2.60","4.50","4.50"]
["","SCOP/A","","","4.60","4.60","4.68","4.68","4.60","4.60"]
["","Annual energy consumption","","kWh/a","792","792","777","777","1,369","1,369"]