{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":25,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / 2MXM-A9"]
[]
[]
[]
[]
["","","","","FTXM20N2V1B / FTXM25N2V1B / 2MXM40A2V1B9","FTXM20N2V1B / FTXM35N2V1B / 2MXM40A2V1B9","FTXM25N2V1B / FTXM35N2V1B / 2MXM40A2V1B9","FTXM25N2V1B / FTXM25N2V1B / 2MXM40A2V1B9","FTXM20N2V1B / FTXM20N2V1B / 2MXM40A2V1B9","FTXM25N2V1B / FTXM25N2V1B / 2MXM50A2V1B9","FTXM20N2V1B / FTXM20N2V1B / 2MXM50A2V1B9","FTXM20N2V1B / FTXM50N2V1B / 2MXM50A2V1B9","FTXM20N2V1B / FTXM42N2V1B / 2MXM50A2V1B9","FTXM25N2V1B / FTXM35N2V1B / 2MXM50A2V1B9","FTXM25N2V1B / FTXM42N2V1B / 2MXM50A2V1B9","FTXM20N2V1B / FTXM25N2V1B / 2MXM50A2V1B9","FTXM20N2V1B / FTXM35N2V1B / 2MXM50A2V1B9","FTXM42N2V1B / FTXM42N2V1B / 2MXM50A2V1B9","FTXM25N2V1B / FTXM50N2V1B / 2MXM50A2V1B9","FTXM35N2V1B / FTXM35N2V1B / 2MXM50A2V1B9","FTXM35N2V1B / FTXM42N2V1B / 2MXM50A2V1B9","FTXM35N2V1B / FTXM50N2V1B / 2MXM50A2V1B9","FTXM20N2V1B / FTXM50N2V1B / 2MXM68A2V1B9","FTXM25N2V1B / FTXM42N2V1B / 2MXM68A2V1B9","FTXM35N2V1B / FTXM35N2V1B / 2MXM68A2V1B9"]
["Cooling capacity","Nom.","","kW","4.00","4.00","4.00","4.00"]
["Heating capacity","Nom.","","kW","4.20","4.20","4.20","4.20"]
["Nominal efficiency","Annual energy consumption","","kWh","481","476","472","478"]
["","COP","","","4.32","4.41","4.46","4.37"]
["","EER","","","4.16","4.20","4.24","4.18"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","A","A","A","A"]
["Space cooling","Annual energy consumption","","kWh/a","165","171","173","168"]
["","Energy efficiency class","","","A+++","A++","A++","A++"]
["","Capacity","Pdesign","kW","4.00","4.00","4.00","4.00"]
["","SEER","","","8.50","8.19","8.11","8.36"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","973","974","971","974"]
["","Capacity","Pdesign","kW","3.20","3.20","3.20","3.20"]
["","Energy efficiency class","","","A++","A++","A++","A++"]
["","Pdh Heating capacity at -10°","","kW","2.56","2.58","2.59","2.57"]
["","SCOP/A","","","4.60","4.60","4.61","4.60"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Cooling capacity","Nom.","","kW","","","","","4.00","5.00","4.00","5.00","5.00","5.00","5.00","4.50","5.00","5.00","5.00","5.00","5.00","5.00","6.8","6.7","6.8"]
["Heating capacity","Nom.","","kW","","","","","4.20","5.60","5.20","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","8.60","8.30","8.60"]
["Nominal efficiency","EER","","","","","","","4.30","4.01","4.25","4.11","4.07","4.06","4.09","4.21","4.04","4.16","4.13","4.11","4.14","4.18","3.59","3.74","3.94"]
["","COP","","","","","","","4.28","4.08","4.09","4.15","4.13","4.05","4.03","4.10","4.12","3.98","3.98","4.01","4.00","3.94","3.82","3.95","3.81"]
["","Annual energy consumption","","kWh","","","","","465","623","471","608","614","616","611","534","619","601","605","608","604","598","947","896","863"]
["","Energy labeling Directive","Cooling","","","","","","A","A","A","A","A","A","A","A","A","A","A","A","A","A"]
["","","Heating","","","","","","A","A","A","A","A","A","A","A","A","A","A","A","A","A"]
["Space cooling","Energy efficiency class","","","","","","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A++","A++","A++"]
["","Capacity","Pdesign","kW","","","","","4.00","5.00","4.00","5.00","5.00","5.00","5.00","4.50","5.00","5.00","5.00","5.00","5.00","5.00","6.80","6.70","6.80"]
["","SEER","","","","","","","8.53","8.53","8.71","8.51","8.54","8.56","8.58","8.68","8.54","8.57","8.52","8.58","8.60","8.53","6.75","6.94","6.97"]
["","Annual energy consumption","","kWh/a","","","","","164","205","161","206","205","204","204","181","205","204","205","204","203","205","353","338","342"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A","A","A+"]
["","Capacity","Pdesign","kW","","","","","3.20","4.20","4.00","4.20","4.20","4.20","4.20","4.10","4.20","4.20","4.20","4.20","4.20","4.20","4.50","4.30","4.80"]
["","SCOP/A","","","","","","","4.64","4.61","4.61","4.66","4.61","4.62","4.65","4.61","4.61","4.67","4.69","4.63","4.64","4.73","3.90","3.86","4.00"]
["","Pdh Heating capacity at -10°","","kW","","","","","2.55","3.20","2.81","3.17","2.88","2.89","2.91","2.83","2.86","2.97","3.21","2.93","2.95","3.25","3.55","3.41","3.73"]
["","Annual energy consumption","","kWh/a","","","","","966","1275","1216","1261","1277","1272","1265","1246","1275","1259","1255","1269","1266","1243","1614","1560","1680"]
["Опсег на енергетска ефикасност","","","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]