{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BB"]
[]
[]
[]
[]
["","","","","","FTXTA30B2V1BB"]
["Sound pressure level","Heating","","High","dBA","41"]
["","","","Medium","dBA","31"]
["","","","Silent operation","dBA","19"]
["","","","Low","dBA","24"]
["","Cooling","","Medium","dBA","32"]
["","","","Silent operation","dBA","20"]
["","","","Low","dBA","25"]
["","","","High","dBA","43"]
["Standard Accessories","Прирачник за инсталирање","","","","1"]
["","Прирачник за работа","","","","1"]
["","Филтер за воздух","","","","2"]
["","Инфрацрвен далечински управувач","","","","1"]
["","Монтажна плочка за далечински управувач","","","","1"]
["","Кесичка со завртки","","","","1"]
["","Капак за завртка","","","","2"]
["","AAA-батерии со суви ќелии","","","","2"]
["","Општи безбедносни мерки","","","","1"]
["Refrigerant","GWP","","","","675.0"]
["Control systems","Жичен далечински управувач","","","","BRC073A4"]
["","Infrared remote control","","","","ARC466A59"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","OD","mm","9.50"]
["","Drain","","","","18"]
["Power input","Cooling","","Nom.","kW","0.023"]
["","Heating","","Nom.","kW","0.022"]
["Sound power level","Cooling","","","dBA","60"]
["","Heating","","","dBA","60"]
["Dimensions","Unit","","Ширина","mm","798"]
["","","","Длабочина","mm","189"]
["","","","Висина","mm","295"]
["Casing","Colour","","","","Black"]
["Weight","Единица","","","kg","11.5"]
["Fan","Air flow rate","Heating","High","m³/min","11.5"]
["","","","Low","m³/min","6.0"]
["","","","Medium","m³/min","8.0"]
["","","","Silent operation","m³/min","5.1"]
["","","Cooling","Low","m³/min","5.7"]
["","","","Medium","m³/min","8.3"]
["","","","High","m³/min","11.9"]
["","","","Silent operation","m³/min","4.6"]
["Power supply","Фаза","","","","1~"]
["","Frequency","","","Hz","50"]
["","Име","","","","V1"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","","(3) - See separate drawing for electrical data"]