{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A9 / RXTP-R"]
[]
[]
[]
[]
["","","","","FVXM25A3V1B9 / RXTP25R2V1B","FVXM35A3V1B9 / RXTP35R2V1B"]
["Cooling capacity","Min.","","kW","1.40","1.40"]
["","Nom.","","kW","2.50","3.50"]
["","Max.","","kW","4.20","4.30"]
["Heating capacity","Min.","","kW","1.20","1.20"]
["","Nom.","","kW","3.20","4.00"]
["","Max.","","kW","5.70","6.20"]
["Nominal efficiency","Annual energy consumption","","kWh","328","510"]
["","COP","","","3.86","3.54"]
["","EER","","","3.81","3.43"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","B"]
["Space cooling","Annual energy consumption","","kWh/a","135","201"]
["","Energy efficiency class","","","A++","A++"]
["","Capacity","Pdesign","kW","2.50","3.50"]
["","SEER","","","6.50","6.10"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","744","909"]
["","Capacity","Pdesign","kW","2.50","3.00"]
["","Energy efficiency class","","","A++","A++"]
["","Pdh Heating capacity at -10°","","kW","2.50","3.00"]
["","SCOP/A","","","4.70","4.62"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]
["","","","","(4) - See separate drawing for operation range","(4) - See separate drawing for operation range"]