{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-B / RXM-A9"]
[]
[]
[]
[]
["","","","","FVXM25B2V1B / RXM25A5V1B9","FVXM35B2V1B / RXM35A5V1B9","FVXM50B2V1B / RXM50A5V1B9"]
["Cooling capacity","Min.","","kW","1.3","1.4","1.4"]
["","Nom.","","kW","2.4","3.4","5"]
["","Max.","","kW","3.5","4","5.8"]
["Heating capacity","Min.","","kW","1.3","1.4","1.4"]
["","Nom.","","kW","3.4","4.5","5.8"]
["","Max.","","kW","4.7","5.8","8.1"]
["Nominal efficiency","EER","","","4.63","4.23","3.81"]
["","COP","","","4.55","3.92","3.81"]
["","Annual energy consumption","","kWh","259","402","656"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","A","A","A"]
["Space cooling","Energy efficiency class","","","A+++","A++","A++"]
["","Capacity","Pdesign","kW","2.4","3.4","5"]
["","SEER","","","8.64","8.19","7.3"]
["","Annual energy consumption","","kWh/a","97","145","240"]
["Space heating (Average climate)","Energy efficiency class","","","A++","A++","A+"]
["","Capacity","Pdesign","kW","2.3","2.8","4.1"]
["","SCOP/A","","","4.7","4.68","4.31"]
["","Pdh Heating capacity at -10°","","kW","1.91","2.12","3.56"]
["","Annual energy consumption","","kWh/a","686","837","1330"]
["Опсег на енергетска ефикасност","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]