{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":6,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-B"]
[]
[]
[]
[]
["","","","","","FVXTM30B2V1B"]
["Power input","Cooling","","Nom.","kW","0.02"]
["","Heating","","Nom.","kW","0.03"]
["Куќиште","Боја","","","","Бела"]
["Димензии","Единица","","Висина","mm","600"]
["","","","Ширина","mm","750"]
["","","","Длабочина","mm","238"]
["Тежина","Единица","","","kg","17"]
["Fan","Air flow rate","Cooling","High","m³/min","9"]
["","","","Medium","m³/min","6.7"]
["","","","Low","m³/min","4.8"]
["","","","Silent operation","m³/min","4"]
["","","Heating","High","m³/min","9.4"]
["","","","Medium","m³/min","6.8"]
["","","","Low","m³/min","5.3"]
["","","","Silent operation","m³/min","4"]
["Sound power level","Cooling","","","dBA","53"]
["","Heating","","","dBA","53"]
["Sound pressure level","Cooling","","High","dBA","39"]
["","","","Medium","dBA","32"]
["","","","Low","dBA","25"]
["","","","Silent operation","dBA","20"]
["","Heating","","High","dBA","39"]
["","","","Medium","dBA","32"]
["","","","Low","dBA","25"]
["","","","Silent operation","dBA","19"]
["Разладно средство","GWP","","","","675"]
["Поврзувања на цевките","Течност","","OD","mm","6.35"]
["","Гас","","OD","mm","9.5"]
["","Одвод","","","","VP20 (I.D. 20/O.D. 26)"]
["Контролни системи","Инфрацрвен далечински управувач","","","","ARC466A90"]
["","Жичен далечински управувач","","","","BRC073A1"]
["Standard Accessories","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Напојување со струја","Име","","","","V1"]
["","Фаза","","","","1~"]
["Power supply","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","","(3) - See separate drawing for electrical data"]