{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-B9"]
[]
[]
[]
[]
["","","","","","RXA42B5V1B9"]
["Димензии","Единица","","Висина","mm","734"]
["","","","Ширина","mm","954"]
["","","","Длабочина","mm","401"]
["Тежина","Единица","","","kg","49"]
["Компресор","Тип","","","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10"]
["","","","Max.","°CDB","46"]
["","Heating","Ambient","Min.","°CWB","-15"]
["","","","Max.","°CWB","18"]
["Sound pressure level","Cooling","","Nom.","dBA","48"]
["","Heating","","Nom.","dBA","48"]
["Разладно средство","Тип","","","","R-32"]
["","Полнење","","","kg","1.1"]
["Refrigerant","Charge","","","tCO2Eq","0.75"]
["Разладно средство","GWP","","","","675"]
["Piping connections","Piping length","OU - IU","Max.","m","30"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","20"]
["Standard Accessories","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain cap","","","","3"]
["","Drain plug","","","","1"]
["Опсег на енергетска ефикасност","","","","","A+++ ~ D"]
["Напојување со струја","Фаза","","","","1~"]
["Power supply","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - See separate drawing for operation range"]
["","","","","","(2) - See separate drawing for electrical data"]
["","","","","","(3) - Contains fluorinated greenhouse gases"]