{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-CB"]
[]
[]
[]
[]
["","","","","","CTXA15C2V1BB"]
["Power input","Cooling","","Nom.","kW","0.020"]
["","Heating","","Nom.","kW","0.020"]
["Casing","Colour","","","","Black"]
["Dimensions","Unit","","Висина","mm","295"]
["","","","Width","mm","798"]
["","","","Depth","mm","189"]
["Weight","Единица","","","kg","11.5"]
["Fan","Air flow rate","Cooling","High","m³/min","11.0"]
["","","","Medium","m³/min","8.2"]
["","","","Low","m³/min","6.1"]
["","","","Silent operation","m³/min","4.6"]
["","","Heating","High","m³/min","10.9"]
["","","","Medium","m³/min","8.7"]
["","","","Low","m³/min","6.4"]
["","","","Silent operation","m³/min","4.5"]
["Sound power level","Cooling","","","dBA","57"]
["Sound pressure level","Cooling","","High","dBA","39"]
["","","","Medium","dBA","32"]
["","","","Low","dBA","25"]
["","","","Silent operation","dBA","21"]
["","Heating","","High","dBA","39"]
["","","","Medium","dBA","32"]
["","","","Low","dBA","25"]
["","","","Silent operation","dBA","21"]
["Refrigerant","GWP","","","","675.0"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","OD","mm","9.50"]
["","Drain","","","","18"]
["Control systems","Infrared remote control","","","","ARC466A85"]
["","Wired remote control","","","","BRC073A1"]
["Standard Accessories","Прирачник за инсталирање","","","","1"]
["","Прирачник за работа","","","","1"]
["","Филтер за воздух","","","","2"]
["","Инфрацрвен далечински управувач","","","","1"]
["","Монтажна плочка за далечински управувач","","","","1"]
["","Кесичка со завртки","","","","1"]
["","Капак за завртка","","","","2"]
["","AAA-батерии со суви ќелии","","","","2"]
["","Општи безбедносни мерки","","","","1"]
["Power supply","Name","","","","V1"]
["","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]