{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CW"]
[]
[]
[]
[]
["","","","","","FTXTA30C2V1BW"]
["Power input","Cooling","","Nom.","kW","0.023"]
["","Heating","","Nom.","kW","0.022"]
["Куќиште","Боја","","","","Бела"]
["Димензии","Единица","","Висина","mm","295"]
["","","","Ширина","mm","798"]
["","","","Длабочина","mm","189"]
["Тежина","Единица","","","kg","12"]
["Fan","Air flow rate","Cooling","High","m³/min","13.1"]
["","","","Medium","m³/min","9"]
["","","","Low","m³/min","6"]
["","","","Silent operation","m³/min","4.9"]
["","","Heating","High","m³/min","12.3"]
["","","","Medium","m³/min","8.2"]
["","","","Low","m³/min","5.8"]
["","","","Silent operation","m³/min","5"]
["Sound power level","Cooling","","","dBA","60"]
["","Heating","","","dBA","60"]
["Sound pressure level","Cooling","","High","dBA","43"]
["","","","Medium","dBA","32"]
["","","","Low","dBA","25"]
["","","","Silent operation","dBA","20"]
["","Heating","","High","dBA","41"]
["","","","Medium","dBA","31"]
["","","","Low","dBA","24"]
["","","","Silent operation","dBA","19"]
["Разладно средство","GWP","","","","675"]
["Поврзувања на цевките","Течност","","OD","mm","6.35"]
["","Гас","","OD","mm","9.5"]
["","Одвод","","","","18"]
["Control systems","Инфрацрвен далечински управувач","","","","ARC466A84"]
["Контролни системи","Жичен далечински управувач","","","","BRC073A4"]
["Standard Accessories","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Напојување со струја","Фаза","","","","1~"]
["Power supply","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]