{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Sound pressure level","Heating","","High","dBA","45.0"]
["","","","Medium","dBA","31.0"]
["","","","Silent operation","dBA","19.0"]
["","","","Low","dBA","22.0"]
["","Cooling","","Medium","dBA","33.0"]
["","","","Silent operation","dBA","21.0"]
["","","","Low","dBA","25.0"]
["","","","High","dBA","45.0"]
["Standard Accessories","Прирачник за инсталирање","","","","1"]
["","Прирачник за работа","","","","1"]
["","Безжичен далечински управувач","","","","1"]
["","AAA-батерии со суви ќелии","","","","2"]
["","Држач за далечински управувач","","","","1"]
["","Монтажна плочка","","","","1"]
["","Завртки за фиксирање на внатрешната единица","","","","2"]
["","Филтер за сребрени честички","","","","1"]
["Control systems","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","OD","mm","9.50"]
["","Drain","","","","18"]
["Power input","Cooling","","Nom.","kW","0.035"]
["","Heating","","Nom.","kW","0.039"]
["Sound power level","Cooling","","","dBA","60.0"]
["","Heating","","","dBA","61.0"]
["Dimensions","Unit","","Ширина","mm","778"]
["","","","Длабочина","mm","272"]
["","","","Висина","mm","295"]
["Casing","Colour","","","","White"]
["Weight","Единица","","","kg","10.0"]
["Fan","Air flow rate","Heating","High","m³/min","12.5"]
["","","","Low","m³/min","4.9"]
["","","","Medium","m³/min","7.5"]
["","","","Silent operation","m³/min","4.0"]
["","","Cooling","Low","m³/min","5.3"]
["","","","Medium","m³/min","7.8"]
["","","","High","m³/min","12.2"]
["","","","Silent operation","m³/min","4.1"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Име","","","","V1"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","","(3) - See separate drawings for electrical data"]
["Power input","Cooling","","Nom.","kW","","0.053"]
["","Heating","","Nom.","kW","","0.06"]
["Куќиште","Боја","","","","","Бела"]
["Димензии","Единица","","Висина","mm","","299"]
["","","","Ширина","mm","","998"]
["","","","Длабочина","mm","","292"]
["Тежина","Единица","","","kg","","14.5"]
["Fan","Air flow rate","Cooling","High","m³/min","","15.4"]
["","","","Medium","m³/min","","9.5"]
["","","","Low","m³/min","","5.8"]
["","","","Silent operation","m³/min","","4.6"]
["","","Heating","High","m³/min","","17.5"]
["","","","Medium","m³/min","","10.5"]
["","","","Low","m³/min","","7.1"]
["","","","Silent operation","m³/min","","5.9"]
["Sound power level","Cooling","","","dBA","","60"]
["","Heating","","","dBA","","61"]
["Sound pressure level","Cooling","","High","dBA","","46"]
["","","","Medium","dBA","","32"]
["","","","Low","dBA","","24"]
["","","","Silent operation","dBA","","20"]
["","Heating","","High","dBA","","46"]
["","","","Medium","dBA","","31"]
["","","","Low","dBA","","22"]
["","","","Silent operation","dBA","","19"]
["Поврзувања на цевките","Течност","","OD","mm","","6.35"]
["","Гас","","OD","mm","","9.5"]
["","Одвод","","","","","18"]
["Control systems","Infrared remote control","","","","","ARC466A75"]
["Контролни системи","Жичен далечински управувач","","","","","BRC073A1"]
["Standard Accessories","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Напојување со струја","Име","","","","","V1"]
["","Фаза","","","","","1~"]
["Power supply","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]