{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-N"]
[]
[]
[]
[]
["","","","","","FTXTP25N5V1B","FTXTP35N5V1B"]
["Power input","Cooling","","Nom.","kW","0.032","0.032"]
["","Heating","","Nom.","kW","0.032","0.032"]
["Куќиште","Боја","","","","Бела","Бела"]
["Димензии","Единица","","Висина","mm","286","286"]
["","","","Ширина","mm","770","770"]
["","","","Длабочина","mm","225","225"]
["Тежина","Единица","","","kg","9","9"]
["Fan","Air flow rate","Cooling","High","m³/min","11","11"]
["","","","Medium","m³/min","7.9","7.9"]
["","","","Low","m³/min","5","5"]
["","","","Silent operation","m³/min","3.7","3.7"]
["","","Heating","High","m³/min","10.5","10.5"]
["","","","Medium","m³/min","9","9"]
["","","","Low","m³/min","5.5","5.5"]
["","","","Silent operation","m³/min","4.4","4.4"]
["Sound power level","Cooling","","","dBA","58","58"]
["","Heating","","","dBA","58","58"]
["Sound pressure level","Cooling","","High","dBA","43","43"]
["","","","Medium","dBA","35","35"]
["","","","Low","dBA","26","26"]
["","","","Silent operation","dBA","21","21"]
["","Heating","","High","dBA","43","43"]
["","","","Medium","dBA","35","35"]
["","","","Low","dBA","26","26"]
["","","","Silent operation","dBA","21","21"]
["Разладно средство","GWP","","","","675","675"]
["Поврзувања на цевките","Течност","","OD","mm","6.35","6.35"]
["","Гас","","OD","mm","9.5","9.5"]
["","Одвод","","","","18","18"]
["Control systems","Инфрацрвен далечински управувач","","","","ARC480A53","ARC480A53"]
["Контролни системи","Жичен далечински управувач","","","","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Напојување со струја","Фаза","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]